/*
** Linker script for PIC24FJ128GA010
*/

OUTPUT_ARCH("24FJ128GA010")
EXTERN(__resetPRI)
EXTERN(__resetALT)


/*
** Memory Regions
*/
MEMORY
{
  data  (a!xr) : ORIGIN = 0x800,         LENGTH = 0x2000
  reset        : ORIGIN = 0x0,           LENGTH = 0x4
  ivt          : ORIGIN = 0x4,           LENGTH = 0xFC
  aivt         : ORIGIN = 0x104,         LENGTH = 0xFC
  program (xr) : ORIGIN = 0x200,         LENGTH = 0x155FC
  config2      : ORIGIN = 0x157FC,       LENGTH = 0x2
  config1      : ORIGIN = 0x157FE,       LENGTH = 0x2
}
__IVT_BASE  = 0x4;
__AIVT_BASE = 0x104;
__DATA_BASE = 0x800;
__CODE_BASE = 0x200;


/*
** ==================== Section Map ======================
*/
SECTIONS
{
  /*
  ** ========== Program Memory ==========
  */


  /*
  ** Reset Instruction
  */
  .reset :
  {
        SHORT(ABSOLUTE(__reset));
        SHORT(0x04);
        SHORT((ABSOLUTE(__reset) >> 16) & 0x7F);
        SHORT(0);
  } >reset


  /*
  ** Interrupt Vector Tables
  **
  ** The primary and alternate tables are loaded
  ** here, between sections .reset and .text.
  ** Vector table source code appears below.
  */


  /*
  ** User Code and Library Code
  */
  .text __CODE_BASE :
  {
        *(.handle);
        *(.libc) *(.libm) *(.libdsp);  /* keep together in this order */
        *(.lib*);
        *(.text);
  } >program


  /*
  ** Configuration Words
  */
  __CONFIG2 :
  { *(__CONFIG2.sec)    } >config2
  __CONFIG1 :
  { *(__CONFIG1.sec)    } >config1


  /*
  ** =========== Data Memory ===========
  */


  /*
  ** ICD Debug Exec
  **
  ** This section provides optional storage for
  ** the ICD2 debugger. Define a global symbol
  ** named __ICD2RAM to enable ICD2. This section
  ** must be loaded at data address 0x800.
  */
  .icd __DATA_BASE (NOLOAD):
  {
    . += (DEFINED (__ICD2RAM) ? 0x50 : 0 );
  } > data


  /*
  ** Other sections in data memory are not explicitly mapped.
  ** Instead they are allocated according to their section
  ** attributes, which is most efficient.
  ** 
  ** If a specific arrangement of sections is required
  ** (other than what can be achieved using attributes)
  ** additional sections may be defined here. See chapter
  ** 10.5 in the MPLAB ASM30/LINK30 User's Guide (DS51317)
  ** for more information.
  */


  /*
  ** ========== Debug Info ==============
  */

  .comment        0 : { *(.comment) }

  /*
  ** DWARF-2
  */
  .debug_info     0 : { *(.debug_info) *(.gnu.linkonce.wi.*) }
  .debug_abbrev   0 : { *(.debug_abbrev) }
  .debug_line     0 : { *(.debug_line) }
  .debug_frame    0 : { *(.debug_frame) }
  .debug_str      0 : { *(.debug_str) }
  .debug_loc      0 : { *(.debug_loc) }
  .debug_macinfo  0 : { *(.debug_macinfo) }
  .debug_pubnames 0 : { *(.debug_pubnames) }
  .debug_ranges   0 : { *(.debug_ranges) }
  .debug_aranges  0 : { *(.debug_aranges) }

} /* SECTIONS */

/*
** ================= End of Section Map ================
*/

/*
** Section Map for Interrupt Vector Tables
*/
SECTIONS
{

/*
** Interrupt Vector Table
*/
.ivt __IVT_BASE :
  {
    LONG( DEFINED(__ReservedTrap0)    ? ABSOLUTE(__ReservedTrap0)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OscillatorFail)    ? ABSOLUTE(__OscillatorFail)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__AddressError)    ? ABSOLUTE(__AddressError)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__StackError)    ? ABSOLUTE(__StackError)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__MathError)    ? ABSOLUTE(__MathError)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__ReservedTrap5)    ? ABSOLUTE(__ReservedTrap5)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__ReservedTrap6)    ? ABSOLUTE(__ReservedTrap6)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__ReservedTrap7)    ? ABSOLUTE(__ReservedTrap7)    :
         ABSOLUTE(__DefaultInterrupt));

    LONG( DEFINED(__INT0Interrupt)    ? ABSOLUTE(__INT0Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__IC1Interrupt)    ? ABSOLUTE(__IC1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OC1Interrupt)    ? ABSOLUTE(__OC1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__T1Interrupt)    ? ABSOLUTE(__T1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt4)    ? ABSOLUTE(__Interrupt4)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__IC2Interrupt)    ? ABSOLUTE(__IC2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OC2Interrupt)    ? ABSOLUTE(__OC2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__T2Interrupt)    ? ABSOLUTE(__T2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__T3Interrupt)    ? ABSOLUTE(__T3Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SPI1ErrInterrupt)    ? ABSOLUTE(__SPI1ErrInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SPI1TInterrupt)    ? ABSOLUTE(__SPI1TInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U1RXInterrupt)    ? ABSOLUTE(__U1RXInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U1TXInterrupt)    ? ABSOLUTE(__U1TXInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__ADC1Interrupt)    ? ABSOLUTE(__ADC1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt14)    ? ABSOLUTE(__Interrupt14)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt15)    ? ABSOLUTE(__Interrupt15)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SI2C1Interrupt)    ? ABSOLUTE(__SI2C1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__MI2C1Interrupt)    ? ABSOLUTE(__MI2C1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__CompInterrupt)    ? ABSOLUTE(__CompInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__CNInterrupt)    ? ABSOLUTE(__CNInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__INT1Interrupt)    ? ABSOLUTE(__INT1Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt21)    ? ABSOLUTE(__Interrupt21)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt22)    ? ABSOLUTE(__Interrupt22)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt23)    ? ABSOLUTE(__Interrupt23)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt24)    ? ABSOLUTE(__Interrupt24)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OC3Interrupt)    ? ABSOLUTE(__OC3Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OC4Interrupt)    ? ABSOLUTE(__OC4Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__T4Interrupt)    ? ABSOLUTE(__T4Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__T5Interrupt)    ? ABSOLUTE(__T5Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__INT2Interrupt)    ? ABSOLUTE(__INT2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U2RXInterrupt)    ? ABSOLUTE(__U2RXInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U2TXInterrupt)    ? ABSOLUTE(__U2TXInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SPI2ErrInterrupt)    ? ABSOLUTE(__SPI2ErrInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SPI2Interrupt)    ? ABSOLUTE(__SPI2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt34)    ? ABSOLUTE(__Interrupt34)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt35)    ? ABSOLUTE(__Interrupt35)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt36)    ? ABSOLUTE(__Interrupt36)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__IC3Interrupt)    ? ABSOLUTE(__IC3Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__IC4Interrupt)    ? ABSOLUTE(__IC4Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__IC5Interrupt)    ? ABSOLUTE(__IC5Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt40)    ? ABSOLUTE(__Interrupt40)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__OC5Interrupt)    ? ABSOLUTE(__OC5Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt42)    ? ABSOLUTE(__Interrupt42)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt43)    ? ABSOLUTE(__Interrupt43)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt44)    ? ABSOLUTE(__Interrupt44)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__PMPInterrupt)    ? ABSOLUTE(__PMPInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt46)    ? ABSOLUTE(__Interrupt46)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt47)    ? ABSOLUTE(__Interrupt47)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt48)    ? ABSOLUTE(__Interrupt48)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__SI2C2Interrupt)    ? ABSOLUTE(__SI2C2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__MI2C2Interrupt)    ? ABSOLUTE(__MI2C2Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt51)    ? ABSOLUTE(__Interrupt51)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt52)    ? ABSOLUTE(__Interrupt52)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__INT3Interrupt)    ? ABSOLUTE(__INT3Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__INT4Interrupt)    ? ABSOLUTE(__INT4Interrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt55)    ? ABSOLUTE(__Interrupt55)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt56)    ? ABSOLUTE(__Interrupt56)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt57)    ? ABSOLUTE(__Interrupt57)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt58)    ? ABSOLUTE(__Interrupt58)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt59)    ? ABSOLUTE(__Interrupt59)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt60)    ? ABSOLUTE(__Interrupt60)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt61)    ? ABSOLUTE(__Interrupt61)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__RTCCInterrupt)    ? ABSOLUTE(__RTCCInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt63)    ? ABSOLUTE(__Interrupt63)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt64)    ? ABSOLUTE(__Interrupt64)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U1ErrInterrupt)    ? ABSOLUTE(__U1ErrInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__U2ErrInterrupt)    ? ABSOLUTE(__U2ErrInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__CRCInterrupt)    ? ABSOLUTE(__CRCInterrupt)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt68)    ? ABSOLUTE(__Interrupt68)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt69)    ? ABSOLUTE(__Interrupt69)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt70)    ? ABSOLUTE(__Interrupt70)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt71)    ? ABSOLUTE(__Interrupt71)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt72)    ? ABSOLUTE(__Interrupt72)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt73)    ? ABSOLUTE(__Interrupt73)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt74)    ? ABSOLUTE(__Interrupt74)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt75)    ? ABSOLUTE(__Interrupt75)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt76)    ? ABSOLUTE(__Interrupt76)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt77)    ? ABSOLUTE(__Interrupt77)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt78)    ? ABSOLUTE(__Interrupt78)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt79)    ? ABSOLUTE(__Interrupt79)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt80)    ? ABSOLUTE(__Interrupt80)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt81)    ? ABSOLUTE(__Interrupt81)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt82)    ? ABSOLUTE(__Interrupt82)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt83)    ? ABSOLUTE(__Interrupt83)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt84)    ? ABSOLUTE(__Interrupt84)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt85)    ? ABSOLUTE(__Interrupt85)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt86)    ? ABSOLUTE(__Interrupt86)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt87)    ? ABSOLUTE(__Interrupt87)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt88)    ? ABSOLUTE(__Interrupt88)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt89)    ? ABSOLUTE(__Interrupt89)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt90)    ? ABSOLUTE(__Interrupt90)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt91)    ? ABSOLUTE(__Interrupt91)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt92)    ? ABSOLUTE(__Interrupt92)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt93)    ? ABSOLUTE(__Interrupt93)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt94)    ? ABSOLUTE(__Interrupt94)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt95)    ? ABSOLUTE(__Interrupt95)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt96)    ? ABSOLUTE(__Interrupt96)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt97)    ? ABSOLUTE(__Interrupt97)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt98)    ? ABSOLUTE(__Interrupt98)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt99)    ? ABSOLUTE(__Interrupt99)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt100)    ? ABSOLUTE(__Interrupt100)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt101)    ? ABSOLUTE(__Interrupt101)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt102)    ? ABSOLUTE(__Interrupt102)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt103)    ? ABSOLUTE(__Interrupt103)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt104)    ? ABSOLUTE(__Interrupt104)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt105)    ? ABSOLUTE(__Interrupt105)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt106)    ? ABSOLUTE(__Interrupt106)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt107)    ? ABSOLUTE(__Interrupt107)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt108)    ? ABSOLUTE(__Interrupt108)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt109)    ? ABSOLUTE(__Interrupt109)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt110)    ? ABSOLUTE(__Interrupt110)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt111)    ? ABSOLUTE(__Interrupt111)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt112)    ? ABSOLUTE(__Interrupt112)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt113)    ? ABSOLUTE(__Interrupt113)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt114)    ? ABSOLUTE(__Interrupt114)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt115)    ? ABSOLUTE(__Interrupt115)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt116)    ? ABSOLUTE(__Interrupt116)    :
         ABSOLUTE(__DefaultInterrupt));
    LONG( DEFINED(__Interrupt117)    ? ABSOLUTE(__Interrupt117)    :
         ABSOLUTE(__DefaultInterrupt));
  } >ivt


/*
** Alternate Interrupt Vector Table
*/
.aivt __AIVT_BASE :
  {
    LONG( DEFINED(__AltReservedTrap0)    ? ABSOLUTE(__AltReservedTrap0)    :
         (DEFINED(__ReservedTrap0)       ? ABSOLUTE(__ReservedTrap0)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOscillatorFail)    ? ABSOLUTE(__AltOscillatorFail)    :
         (DEFINED(__OscillatorFail)       ? ABSOLUTE(__OscillatorFail)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltAddressError)    ? ABSOLUTE(__AltAddressError)    :
         (DEFINED(__AddressError)       ? ABSOLUTE(__AddressError)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltStackError)    ? ABSOLUTE(__AltStackError)    :
         (DEFINED(__StackError)       ? ABSOLUTE(__StackError)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltMathError)    ? ABSOLUTE(__AltMathError)    :
         (DEFINED(__MathError)       ? ABSOLUTE(__MathError)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltReservedTrap5)    ? ABSOLUTE(__AltReservedTrap5)    :
         (DEFINED(__ReservedTrap5)       ? ABSOLUTE(__ReservedTrap5)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltReservedTrap6)    ? ABSOLUTE(__AltReservedTrap6)    :
         (DEFINED(__ReservedTrap6)       ? ABSOLUTE(__ReservedTrap6)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltReservedTrap7)    ? ABSOLUTE(__AltReservedTrap7)    :
         (DEFINED(__ReservedTrap7)       ? ABSOLUTE(__ReservedTrap7)       :
         ABSOLUTE(__DefaultInterrupt)));

    LONG( DEFINED(__AltINT0Interrupt)    ? ABSOLUTE(__AltINT0Interrupt)    :
         (DEFINED(__INT0Interrupt)       ? ABSOLUTE(__INT0Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltIC1Interrupt)    ? ABSOLUTE(__AltIC1Interrupt)    :
         (DEFINED(__IC1Interrupt)       ? ABSOLUTE(__IC1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOC1Interrupt)    ? ABSOLUTE(__AltOC1Interrupt)    :
         (DEFINED(__OC1Interrupt)       ? ABSOLUTE(__OC1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltT1Interrupt)    ? ABSOLUTE(__AltT1Interrupt)    :
         (DEFINED(__T1Interrupt)       ? ABSOLUTE(__T1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt4)    ? ABSOLUTE(__AltInterrupt4)    :
         (DEFINED(__Interrupt4)       ? ABSOLUTE(__Interrupt4)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltIC2Interrupt)    ? ABSOLUTE(__AltIC2Interrupt)    :
         (DEFINED(__IC2Interrupt)       ? ABSOLUTE(__IC2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOC2Interrupt)    ? ABSOLUTE(__AltOC2Interrupt)    :
         (DEFINED(__OC2Interrupt)       ? ABSOLUTE(__OC2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltT2Interrupt)    ? ABSOLUTE(__AltT2Interrupt)    :
         (DEFINED(__T2Interrupt)       ? ABSOLUTE(__T2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltT3Interrupt)    ? ABSOLUTE(__AltT3Interrupt)    :
         (DEFINED(__T3Interrupt)       ? ABSOLUTE(__T3Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSPI1ErrInterrupt)    ? ABSOLUTE(__AltSPI1ErrInterrupt)    :
         (DEFINED(__SPI1ErrInterrupt)       ? ABSOLUTE(__SPI1ErrInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSPI1TInterrupt)    ? ABSOLUTE(__AltSPI1TInterrupt)    :
         (DEFINED(__SPI1TInterrupt)       ? ABSOLUTE(__SPI1TInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU1RXInterrupt)    ? ABSOLUTE(__AltU1RXInterrupt)    :
         (DEFINED(__U1RXInterrupt)       ? ABSOLUTE(__U1RXInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU1TXInterrupt)    ? ABSOLUTE(__AltU1TXInterrupt)    :
         (DEFINED(__U1TXInterrupt)       ? ABSOLUTE(__U1TXInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltADC1Interrupt)    ? ABSOLUTE(__AltADC1Interrupt)    :
         (DEFINED(__ADC1Interrupt)       ? ABSOLUTE(__ADC1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt14)    ? ABSOLUTE(__AltInterrupt14)    :
         (DEFINED(__Interrupt14)       ? ABSOLUTE(__Interrupt14)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt15)    ? ABSOLUTE(__AltInterrupt15)    :
         (DEFINED(__Interrupt15)       ? ABSOLUTE(__Interrupt15)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSI2C1Interrupt)    ? ABSOLUTE(__AltSI2C1Interrupt)    :
         (DEFINED(__SI2C1Interrupt)       ? ABSOLUTE(__SI2C1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltMI2C1Interrupt)    ? ABSOLUTE(__AltMI2C1Interrupt)    :
         (DEFINED(__MI2C1Interrupt)       ? ABSOLUTE(__MI2C1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltCompInterrupt)    ? ABSOLUTE(__AltCompInterrupt)    :
         (DEFINED(__CompInterrupt)       ? ABSOLUTE(__CompInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltCNInterrupt)    ? ABSOLUTE(__AltCNInterrupt)    :
         (DEFINED(__CNInterrupt)       ? ABSOLUTE(__CNInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltINT1Interrupt)    ? ABSOLUTE(__AltINT1Interrupt)    :
         (DEFINED(__INT1Interrupt)       ? ABSOLUTE(__INT1Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt21)    ? ABSOLUTE(__AltInterrupt21)    :
         (DEFINED(__Interrupt21)       ? ABSOLUTE(__Interrupt21)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt22)    ? ABSOLUTE(__AltInterrupt22)    :
         (DEFINED(__Interrupt22)       ? ABSOLUTE(__Interrupt22)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt23)    ? ABSOLUTE(__AltInterrupt23)    :
         (DEFINED(__Interrupt23)       ? ABSOLUTE(__Interrupt23)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt24)    ? ABSOLUTE(__AltInterrupt24)    :
         (DEFINED(__Interrupt24)       ? ABSOLUTE(__Interrupt24)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOC3Interrupt)    ? ABSOLUTE(__AltOC3Interrupt)    :
         (DEFINED(__OC3Interrupt)       ? ABSOLUTE(__OC3Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOC4Interrupt)    ? ABSOLUTE(__AltOC4Interrupt)    :
         (DEFINED(__OC4Interrupt)       ? ABSOLUTE(__OC4Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltT4Interrupt)    ? ABSOLUTE(__AltT4Interrupt)    :
         (DEFINED(__T4Interrupt)       ? ABSOLUTE(__T4Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltT5Interrupt)    ? ABSOLUTE(__AltT5Interrupt)    :
         (DEFINED(__T5Interrupt)       ? ABSOLUTE(__T5Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltINT2Interrupt)    ? ABSOLUTE(__AltINT2Interrupt)    :
         (DEFINED(__INT2Interrupt)       ? ABSOLUTE(__INT2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU2RXInterrupt)    ? ABSOLUTE(__AltU2RXInterrupt)    :
         (DEFINED(__U2RXInterrupt)       ? ABSOLUTE(__U2RXInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU2TXInterrupt)    ? ABSOLUTE(__AltU2TXInterrupt)    :
         (DEFINED(__U2TXInterrupt)       ? ABSOLUTE(__U2TXInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSPI2ErrInterrupt)    ? ABSOLUTE(__AltSPI2ErrInterrupt)    :
         (DEFINED(__SPI2ErrInterrupt)       ? ABSOLUTE(__SPI2ErrInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSPI2Interrupt)    ? ABSOLUTE(__AltSPI2Interrupt)    :
         (DEFINED(__SPI2Interrupt)       ? ABSOLUTE(__SPI2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt34)    ? ABSOLUTE(__AltInterrupt34)    :
         (DEFINED(__Interrupt34)       ? ABSOLUTE(__Interrupt34)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt35)    ? ABSOLUTE(__AltInterrupt35)    :
         (DEFINED(__Interrupt35)       ? ABSOLUTE(__Interrupt35)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt36)    ? ABSOLUTE(__AltInterrupt36)    :
         (DEFINED(__Interrupt36)       ? ABSOLUTE(__Interrupt36)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltIC3Interrupt)    ? ABSOLUTE(__AltIC3Interrupt)    :
         (DEFINED(__IC3Interrupt)       ? ABSOLUTE(__IC3Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltIC4Interrupt)    ? ABSOLUTE(__AltIC4Interrupt)    :
         (DEFINED(__IC4Interrupt)       ? ABSOLUTE(__IC4Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltIC5Interrupt)    ? ABSOLUTE(__AltIC5Interrupt)    :
         (DEFINED(__IC5Interrupt)       ? ABSOLUTE(__IC5Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt40)    ? ABSOLUTE(__AltInterrupt40)    :
         (DEFINED(__Interrupt40)       ? ABSOLUTE(__Interrupt40)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltOC5Interrupt)    ? ABSOLUTE(__AltOC5Interrupt)    :
         (DEFINED(__OC5Interrupt)       ? ABSOLUTE(__OC5Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt42)    ? ABSOLUTE(__AltInterrupt42)    :
         (DEFINED(__Interrupt42)       ? ABSOLUTE(__Interrupt42)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt43)    ? ABSOLUTE(__AltInterrupt43)    :
         (DEFINED(__Interrupt43)       ? ABSOLUTE(__Interrupt43)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt44)    ? ABSOLUTE(__AltInterrupt44)    :
         (DEFINED(__Interrupt44)       ? ABSOLUTE(__Interrupt44)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltPMPInterrupt)    ? ABSOLUTE(__AltPMPInterrupt)    :
         (DEFINED(__PMPInterrupt)       ? ABSOLUTE(__PMPInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt46)    ? ABSOLUTE(__AltInterrupt46)    :
         (DEFINED(__Interrupt46)       ? ABSOLUTE(__Interrupt46)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt47)    ? ABSOLUTE(__AltInterrupt47)    :
         (DEFINED(__Interrupt47)       ? ABSOLUTE(__Interrupt47)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt48)    ? ABSOLUTE(__AltInterrupt48)    :
         (DEFINED(__Interrupt48)       ? ABSOLUTE(__Interrupt48)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltSI2C2Interrupt)    ? ABSOLUTE(__AltSI2C2Interrupt)    :
         (DEFINED(__SI2C2Interrupt)       ? ABSOLUTE(__SI2C2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltMI2C2Interrupt)    ? ABSOLUTE(__AltMI2C2Interrupt)    :
         (DEFINED(__MI2C2Interrupt)       ? ABSOLUTE(__MI2C2Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt51)    ? ABSOLUTE(__AltInterrupt51)    :
         (DEFINED(__Interrupt51)       ? ABSOLUTE(__Interrupt51)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt52)    ? ABSOLUTE(__AltInterrupt52)    :
         (DEFINED(__Interrupt52)       ? ABSOLUTE(__Interrupt52)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltINT3Interrupt)    ? ABSOLUTE(__AltINT3Interrupt)    :
         (DEFINED(__INT3Interrupt)       ? ABSOLUTE(__INT3Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltINT4Interrupt)    ? ABSOLUTE(__AltINT4Interrupt)    :
         (DEFINED(__INT4Interrupt)       ? ABSOLUTE(__INT4Interrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt55)    ? ABSOLUTE(__AltInterrupt55)    :
         (DEFINED(__Interrupt55)       ? ABSOLUTE(__Interrupt55)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt56)    ? ABSOLUTE(__AltInterrupt56)    :
         (DEFINED(__Interrupt56)       ? ABSOLUTE(__Interrupt56)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt57)    ? ABSOLUTE(__AltInterrupt57)    :
         (DEFINED(__Interrupt57)       ? ABSOLUTE(__Interrupt57)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt58)    ? ABSOLUTE(__AltInterrupt58)    :
         (DEFINED(__Interrupt58)       ? ABSOLUTE(__Interrupt58)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt59)    ? ABSOLUTE(__AltInterrupt59)    :
         (DEFINED(__Interrupt59)       ? ABSOLUTE(__Interrupt59)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt60)    ? ABSOLUTE(__AltInterrupt60)    :
         (DEFINED(__Interrupt60)       ? ABSOLUTE(__Interrupt60)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt61)    ? ABSOLUTE(__AltInterrupt61)    :
         (DEFINED(__Interrupt61)       ? ABSOLUTE(__Interrupt61)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltRTCCInterrupt)    ? ABSOLUTE(__AltRTCCInterrupt)    :
         (DEFINED(__RTCCInterrupt)       ? ABSOLUTE(__RTCCInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt63)    ? ABSOLUTE(__AltInterrupt63)    :
         (DEFINED(__Interrupt63)       ? ABSOLUTE(__Interrupt63)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt64)    ? ABSOLUTE(__AltInterrupt64)    :
         (DEFINED(__Interrupt64)       ? ABSOLUTE(__Interrupt64)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU1ErrInterrupt)    ? ABSOLUTE(__AltU1ErrInterrupt)    :
         (DEFINED(__U1ErrInterrupt)       ? ABSOLUTE(__U1ErrInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltU2ErrInterrupt)    ? ABSOLUTE(__AltU2ErrInterrupt)    :
         (DEFINED(__U2ErrInterrupt)       ? ABSOLUTE(__U2ErrInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltCRCInterrupt)    ? ABSOLUTE(__AltCRCInterrupt)    :
         (DEFINED(__CRCInterrupt)       ? ABSOLUTE(__CRCInterrupt)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt68)    ? ABSOLUTE(__AltInterrupt68)    :
         (DEFINED(__Interrupt68)       ? ABSOLUTE(__Interrupt68)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt69)    ? ABSOLUTE(__AltInterrupt69)    :
         (DEFINED(__Interrupt69)       ? ABSOLUTE(__Interrupt69)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt70)    ? ABSOLUTE(__AltInterrupt70)    :
         (DEFINED(__Interrupt70)       ? ABSOLUTE(__Interrupt70)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt71)    ? ABSOLUTE(__AltInterrupt71)    :
         (DEFINED(__Interrupt71)       ? ABSOLUTE(__Interrupt71)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt72)    ? ABSOLUTE(__AltInterrupt72)    :
         (DEFINED(__Interrupt72)       ? ABSOLUTE(__Interrupt72)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt73)    ? ABSOLUTE(__AltInterrupt73)    :
         (DEFINED(__Interrupt73)       ? ABSOLUTE(__Interrupt73)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt74)    ? ABSOLUTE(__AltInterrupt74)    :
         (DEFINED(__Interrupt74)       ? ABSOLUTE(__Interrupt74)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt75)    ? ABSOLUTE(__AltInterrupt75)    :
         (DEFINED(__Interrupt75)       ? ABSOLUTE(__Interrupt75)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt76)    ? ABSOLUTE(__AltInterrupt76)    :
         (DEFINED(__Interrupt76)       ? ABSOLUTE(__Interrupt76)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt77)    ? ABSOLUTE(__AltInterrupt77)    :
         (DEFINED(__Interrupt77)       ? ABSOLUTE(__Interrupt77)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt78)    ? ABSOLUTE(__AltInterrupt78)    :
         (DEFINED(__Interrupt78)       ? ABSOLUTE(__Interrupt78)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt79)    ? ABSOLUTE(__AltInterrupt79)    :
         (DEFINED(__Interrupt79)       ? ABSOLUTE(__Interrupt79)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt80)    ? ABSOLUTE(__AltInterrupt80)    :
         (DEFINED(__Interrupt80)       ? ABSOLUTE(__Interrupt80)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt81)    ? ABSOLUTE(__AltInterrupt81)    :
         (DEFINED(__Interrupt81)       ? ABSOLUTE(__Interrupt81)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt82)    ? ABSOLUTE(__AltInterrupt82)    :
         (DEFINED(__Interrupt82)       ? ABSOLUTE(__Interrupt82)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt83)    ? ABSOLUTE(__AltInterrupt83)    :
         (DEFINED(__Interrupt83)       ? ABSOLUTE(__Interrupt83)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt84)    ? ABSOLUTE(__AltInterrupt84)    :
         (DEFINED(__Interrupt84)       ? ABSOLUTE(__Interrupt84)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt85)    ? ABSOLUTE(__AltInterrupt85)    :
         (DEFINED(__Interrupt85)       ? ABSOLUTE(__Interrupt85)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt86)    ? ABSOLUTE(__AltInterrupt86)    :
         (DEFINED(__Interrupt86)       ? ABSOLUTE(__Interrupt86)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt87)    ? ABSOLUTE(__AltInterrupt87)    :
         (DEFINED(__Interrupt87)       ? ABSOLUTE(__Interrupt87)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt88)    ? ABSOLUTE(__AltInterrupt88)    :
         (DEFINED(__Interrupt88)       ? ABSOLUTE(__Interrupt88)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt89)    ? ABSOLUTE(__AltInterrupt89)    :
         (DEFINED(__Interrupt89)       ? ABSOLUTE(__Interrupt89)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt90)    ? ABSOLUTE(__AltInterrupt90)    :
         (DEFINED(__Interrupt90)       ? ABSOLUTE(__Interrupt90)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt91)    ? ABSOLUTE(__AltInterrupt91)    :
         (DEFINED(__Interrupt91)       ? ABSOLUTE(__Interrupt91)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt92)    ? ABSOLUTE(__AltInterrupt92)    :
         (DEFINED(__Interrupt92)       ? ABSOLUTE(__Interrupt92)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt93)    ? ABSOLUTE(__AltInterrupt93)    :
         (DEFINED(__Interrupt93)       ? ABSOLUTE(__Interrupt93)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt94)    ? ABSOLUTE(__AltInterrupt94)    :
         (DEFINED(__Interrupt94)       ? ABSOLUTE(__Interrupt94)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt95)    ? ABSOLUTE(__AltInterrupt95)    :
         (DEFINED(__Interrupt95)       ? ABSOLUTE(__Interrupt95)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt96)    ? ABSOLUTE(__AltInterrupt96)    :
         (DEFINED(__Interrupt96)       ? ABSOLUTE(__Interrupt96)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt97)    ? ABSOLUTE(__AltInterrupt97)    :
         (DEFINED(__Interrupt97)       ? ABSOLUTE(__Interrupt97)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt98)    ? ABSOLUTE(__AltInterrupt98)    :
         (DEFINED(__Interrupt98)       ? ABSOLUTE(__Interrupt98)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt99)    ? ABSOLUTE(__AltInterrupt99)    :
         (DEFINED(__Interrupt99)       ? ABSOLUTE(__Interrupt99)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt100)    ? ABSOLUTE(__AltInterrupt100)    :
         (DEFINED(__Interrupt100)       ? ABSOLUTE(__Interrupt100)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt101)    ? ABSOLUTE(__AltInterrupt101)    :
         (DEFINED(__Interrupt101)       ? ABSOLUTE(__Interrupt101)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt102)    ? ABSOLUTE(__AltInterrupt102)    :
         (DEFINED(__Interrupt102)       ? ABSOLUTE(__Interrupt102)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt103)    ? ABSOLUTE(__AltInterrupt103)    :
         (DEFINED(__Interrupt103)       ? ABSOLUTE(__Interrupt103)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt104)    ? ABSOLUTE(__AltInterrupt104)    :
         (DEFINED(__Interrupt104)       ? ABSOLUTE(__Interrupt104)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt105)    ? ABSOLUTE(__AltInterrupt105)    :
         (DEFINED(__Interrupt105)       ? ABSOLUTE(__Interrupt105)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt106)    ? ABSOLUTE(__AltInterrupt106)    :
         (DEFINED(__Interrupt106)       ? ABSOLUTE(__Interrupt106)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt107)    ? ABSOLUTE(__AltInterrupt107)    :
         (DEFINED(__Interrupt107)       ? ABSOLUTE(__Interrupt107)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt108)    ? ABSOLUTE(__AltInterrupt108)    :
         (DEFINED(__Interrupt108)       ? ABSOLUTE(__Interrupt108)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt109)    ? ABSOLUTE(__AltInterrupt109)    :
         (DEFINED(__Interrupt109)       ? ABSOLUTE(__Interrupt109)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt110)    ? ABSOLUTE(__AltInterrupt110)    :
         (DEFINED(__Interrupt110)       ? ABSOLUTE(__Interrupt110)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt111)    ? ABSOLUTE(__AltInterrupt111)    :
         (DEFINED(__Interrupt111)       ? ABSOLUTE(__Interrupt111)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt112)    ? ABSOLUTE(__AltInterrupt112)    :
         (DEFINED(__Interrupt112)       ? ABSOLUTE(__Interrupt112)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt113)    ? ABSOLUTE(__AltInterrupt113)    :
         (DEFINED(__Interrupt113)       ? ABSOLUTE(__Interrupt113)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt114)    ? ABSOLUTE(__AltInterrupt114)    :
         (DEFINED(__Interrupt114)       ? ABSOLUTE(__Interrupt114)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt115)    ? ABSOLUTE(__AltInterrupt115)    :
         (DEFINED(__Interrupt115)       ? ABSOLUTE(__Interrupt115)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt116)    ? ABSOLUTE(__AltInterrupt116)    :
         (DEFINED(__Interrupt116)       ? ABSOLUTE(__Interrupt116)       :
         ABSOLUTE(__DefaultInterrupt)));
    LONG( DEFINED(__AltInterrupt117)    ? ABSOLUTE(__AltInterrupt117)    :
         (DEFINED(__Interrupt117)       ? ABSOLUTE(__Interrupt117)       :
         ABSOLUTE(__DefaultInterrupt)));
  } >aivt
} /* SECTIONS */


/*
** ============== Equates for SFR Addresses =============
*/

 WREG0        = 0x0;
_WREG0        = 0x0;
 WREG1        = 0x2;
_WREG1        = 0x2;
 WREG2        = 0x4;
_WREG2        = 0x4;
 WREG3        = 0x6;
_WREG3        = 0x6;
 WREG4        = 0x8;
_WREG4        = 0x8;
 WREG5        = 0xA;
_WREG5        = 0xA;
 WREG6        = 0xC;
_WREG6        = 0xC;
 WREG7        = 0xE;
_WREG7        = 0xE;
 WREG8        = 0x10;
_WREG8        = 0x10;
 WREG9        = 0x12;
_WREG9        = 0x12;
 WREG10       = 0x14;
_WREG10       = 0x14;
 WREG11       = 0x16;
_WREG11       = 0x16;
 WREG12       = 0x18;
_WREG12       = 0x18;
 WREG13       = 0x1A;
_WREG13       = 0x1A;
 WREG14       = 0x1C;
_WREG14       = 0x1C;
 WREG15       = 0x1E;
_WREG15       = 0x1E;
 SPLIM        = 0x20;
_SPLIM        = 0x20;
 PCL          = 0x2E;
_PCL          = 0x2E;
 PCH          = 0x30;
_PCH          = 0x30;
 TBLPAG       = 0x32;
_TBLPAG       = 0x32;
 PSVPAG       = 0x34;
_PSVPAG       = 0x34;
 RCOUNT       = 0x36;
_RCOUNT       = 0x36;
 SR           = 0x42;
_SR           = 0x42;
_SRbits       = 0x42;
 CORCON       = 0x44;
_CORCON       = 0x44;
_CORCONbits   = 0x44;
 DISICNT      = 0x52;
_DISICNT      = 0x52;
 CNEN1        = 0x60;
_CNEN1        = 0x60;
_CNEN1bits    = 0x60;
 CNEN2        = 0x62;
_CNEN2        = 0x62;
_CNEN2bits    = 0x62;
 CNPU1        = 0x68;
_CNPU1        = 0x68;
_CNPU1bits    = 0x68;
 CNPU2        = 0x6A;
_CNPU2        = 0x6A;
_CNPU2bits    = 0x6A;
 INTCON1      = 0x80;
_INTCON1      = 0x80;
_INTCON1bits  = 0x80;
 INTCON2      = 0x82;
_INTCON2      = 0x82;
_INTCON2bits  = 0x82;
 IFS0         = 0x84;
_IFS0         = 0x84;
_IFS0bits     = 0x84;
 IFS1         = 0x86;
_IFS1         = 0x86;
_IFS1bits     = 0x86;
 IFS2         = 0x88;
_IFS2         = 0x88;
_IFS2bits     = 0x88;
 IFS3         = 0x8A;
_IFS3         = 0x8A;
_IFS3bits     = 0x8A;
 IFS4         = 0x8C;
_IFS4         = 0x8C;
_IFS4bits     = 0x8C;
 IEC0         = 0x94;
_IEC0         = 0x94;
_IEC0bits     = 0x94;
 IEC1         = 0x96;
_IEC1         = 0x96;
_IEC1bits     = 0x96;
 IEC2         = 0x98;
_IEC2         = 0x98;
_IEC2bits     = 0x98;
 IEC3         = 0x9A;
_IEC3         = 0x9A;
_IEC3bits     = 0x9A;
 IEC4         = 0x9C;
_IEC4         = 0x9C;
_IEC4bits     = 0x9C;
 IPC0         = 0xA4;
_IPC0         = 0xA4;
_IPC0bits     = 0xA4;
 IPC1         = 0xA6;
_IPC1         = 0xA6;
_IPC1bits     = 0xA6;
 IPC2         = 0xA8;
_IPC2         = 0xA8;
_IPC2bits     = 0xA8;
 IPC3         = 0xAA;
_IPC3         = 0xAA;
_IPC3bits     = 0xAA;
 IPC4         = 0xAC;
_IPC4         = 0xAC;
_IPC4bits     = 0xAC;
 IPC5         = 0xAE;
_IPC5         = 0xAE;
_IPC5bits     = 0xAE;
 IPC6         = 0xB0;
_IPC6         = 0xB0;
_IPC6bits     = 0xB0;
 IPC7         = 0xB2;
_IPC7         = 0xB2;
_IPC7bits     = 0xB2;
 IPC8         = 0xB4;
_IPC8         = 0xB4;
_IPC8bits     = 0xB4;
 IPC9         = 0xB6;
_IPC9         = 0xB6;
_IPC9bits     = 0xB6;
 IPC10        = 0xB8;
_IPC10        = 0xB8;
_IPC10bits    = 0xB8;
 IPC11        = 0xBA;
_IPC11        = 0xBA;
_IPC11bits    = 0xBA;
 IPC12        = 0xBC;
_IPC12        = 0xBC;
_IPC12bits    = 0xBC;
 IPC13        = 0xBE;
_IPC13        = 0xBE;
_IPC13bits    = 0xBE;
 IPC15        = 0xC2;
_IPC15        = 0xC2;
_IPC15bits    = 0xC2;
 IPC16        = 0xC4;
_IPC16        = 0xC4;
_IPC16bits    = 0xC4;
 TMR1         = 0x100;
_TMR1         = 0x100;
 PR1          = 0x102;
_PR1          = 0x102;
 T1CON        = 0x104;
_T1CON        = 0x104;
_T1CONbits    = 0x104;
 TMR2         = 0x106;
_TMR2         = 0x106;
 TMR3HLD      = 0x108;
_TMR3HLD      = 0x108;
 TMR3         = 0x10A;
_TMR3         = 0x10A;
 PR2          = 0x10C;
_PR2          = 0x10C;
 PR3          = 0x10E;
_PR3          = 0x10E;
 T2CON        = 0x110;
_T2CON        = 0x110;
_T2CONbits    = 0x110;
 T3CON        = 0x112;
_T3CON        = 0x112;
_T3CONbits    = 0x112;
 TMR4         = 0x114;
_TMR4         = 0x114;
 TMR5HLD      = 0x116;
_TMR5HLD      = 0x116;
 TMR5         = 0x118;
_TMR5         = 0x118;
 PR4          = 0x11A;
_PR4          = 0x11A;
 PR5          = 0x11C;
_PR5          = 0x11C;
 T4CON        = 0x11E;
_T4CON        = 0x11E;
_T4CONbits    = 0x11E;
 T5CON        = 0x120;
_T5CON        = 0x120;
_T5CONbits    = 0x120;
 IC1BUF       = 0x140;
_IC1BUF       = 0x140;
 IC1CON       = 0x142;
_IC1CON       = 0x142;
_IC1CONbits   = 0x142;
 IC2BUF       = 0x144;
_IC2BUF       = 0x144;
 IC2CON       = 0x146;
_IC2CON       = 0x146;
_IC2CONbits   = 0x146;
 IC3BUF       = 0x148;
_IC3BUF       = 0x148;
 IC3CON       = 0x14A;
_IC3CON       = 0x14A;
_IC3CONbits   = 0x14A;
 IC4BUF       = 0x14C;
_IC4BUF       = 0x14C;
 IC4CON       = 0x14E;
_IC4CON       = 0x14E;
_IC4CONbits   = 0x14E;
 IC5BUF       = 0x150;
_IC5BUF       = 0x150;
 IC5CON       = 0x152;
_IC5CON       = 0x152;
_IC5CONbits   = 0x152;
 OC1RS        = 0x180;
_OC1RS        = 0x180;
 OC1R         = 0x182;
_OC1R         = 0x182;
 OC1CON       = 0x184;
_OC1CON       = 0x184;
_OC1CONbits   = 0x184;
 OC2RS        = 0x186;
_OC2RS        = 0x186;
 OC2R         = 0x188;
_OC2R         = 0x188;
 OC2CON       = 0x18A;
_OC2CON       = 0x18A;
_OC2CONbits   = 0x18A;
 OC3RS        = 0x18C;
_OC3RS        = 0x18C;
 OC3R         = 0x18E;
_OC3R         = 0x18E;
 OC3CON       = 0x190;
_OC3CON       = 0x190;
_OC3CONbits   = 0x190;
 OC4RS        = 0x192;
_OC4RS        = 0x192;
 OC4R         = 0x194;
_OC4R         = 0x194;
 OC4CON       = 0x196;
_OC4CON       = 0x196;
_OC4CONbits   = 0x196;
 OC5RS        = 0x198;
_OC5RS        = 0x198;
 OC5R         = 0x19A;
_OC5R         = 0x19A;
 OC5CON       = 0x19C;
_OC5CON       = 0x19C;
_OC5CONbits   = 0x19C;
 I2C1RCV      = 0x200;
_I2C1RCV      = 0x200;
 I2C1TRN      = 0x202;
_I2C1TRN      = 0x202;
 I2C1BRG      = 0x204;
_I2C1BRG      = 0x204;
 I2C1CON      = 0x206;
_I2C1CON      = 0x206;
_I2C1CONbits  = 0x206;
 I2C1STAT     = 0x208;
_I2C1STAT     = 0x208;
_I2C1STATbits = 0x208;
 I2C1ADD      = 0x20A;
_I2C1ADD      = 0x20A;
 I2C1MSK      = 0x20C;
_I2C1MSK      = 0x20C;
 I2C2RCV      = 0x210;
_I2C2RCV      = 0x210;
 I2C2TRN      = 0x212;
_I2C2TRN      = 0x212;
 I2C2BRG      = 0x214;
_I2C2BRG      = 0x214;
 I2C2CON      = 0x216;
_I2C2CON      = 0x216;
_I2C2CONbits  = 0x216;
 I2C2STAT     = 0x218;
_I2C2STAT     = 0x218;
_I2C2STATbits = 0x218;
 I2C2ADD      = 0x21A;
_I2C2ADD      = 0x21A;
 I2C2MSK      = 0x21C;
_I2C2MSK      = 0x21C;
 U1MODE       = 0x220;
_U1MODE       = 0x220;
_U1MODEbits   = 0x220;
 U1STA        = 0x222;
_U1STA        = 0x222;
_U1STAbits    = 0x222;
 U1TXREG      = 0x224;
_U1TXREG      = 0x224;
 U1RXREG      = 0x226;
_U1RXREG      = 0x226;
 U1BRG        = 0x228;
_U1BRG        = 0x228;
 U2MODE       = 0x230;
_U2MODE       = 0x230;
_U2MODEbits   = 0x230;
 U2STA        = 0x232;
_U2STA        = 0x232;
_U2STAbits    = 0x232;
 U2TXREG      = 0x234;
_U2TXREG      = 0x234;
 U2RXREG      = 0x236;
_U2RXREG      = 0x236;
 U2BRG        = 0x238;
_U2BRG        = 0x238;
 SPI1STAT     = 0x240;
_SPI1STAT     = 0x240;
_SPI1STATbits = 0x240;
 SPI1CON1     = 0x242;
_SPI1CON1     = 0x242;
_SPI1CON1bits = 0x242;
 SPI1CON2     = 0x244;
_SPI1CON2     = 0x244;
_SPI1CON2bits = 0x244;
 SPI1BUF      = 0x248;
_SPI1BUF      = 0x248;
 SPI2STAT     = 0x260;
_SPI2STAT     = 0x260;
_SPI2STATbits = 0x260;
 SPI2CON1     = 0x262;
_SPI2CON1     = 0x262;
_SPI2CON1bits = 0x262;
 SPI2CON2     = 0x264;
_SPI2CON2     = 0x264;
_SPI2CON2bits = 0x264;
 SPI2BUF      = 0x268;
_SPI2BUF      = 0x268;
 TRISA        = 0x2C0;
_TRISA        = 0x2C0;
_TRISAbits    = 0x2C0;
 PORTA        = 0x2C2;
_PORTA        = 0x2C2;
_PORTAbits    = 0x2C2;
 LATA         = 0x2C4;
_LATA         = 0x2C4;
_LATAbits     = 0x2C4;
 TRISB        = 0x2C6;
_TRISB        = 0x2C6;
_TRISBbits    = 0x2C6;
 PORTB        = 0x2C8;
_PORTB        = 0x2C8;
_PORTBbits    = 0x2C8;
 LATB         = 0x2CA;
_LATB         = 0x2CA;
_LATBbits     = 0x2CA;
 TRISC        = 0x2CC;
_TRISC        = 0x2CC;
_TRISCbits    = 0x2CC;
 PORTC        = 0x2CE;
_PORTC        = 0x2CE;
_PORTCbits    = 0x2CE;
 LATC         = 0x2D0;
_LATC         = 0x2D0;
_LATCbits     = 0x2D0;
 TRISD        = 0x2D2;
_TRISD        = 0x2D2;
_TRISDbits    = 0x2D2;
 PORTD        = 0x2D4;
_PORTD        = 0x2D4;
_PORTDbits    = 0x2D4;
 LATD         = 0x2D6;
_LATD         = 0x2D6;
_LATDbits     = 0x2D6;
 TRISE        = 0x2D8;
_TRISE        = 0x2D8;
_TRISEbits    = 0x2D8;
 PORTE        = 0x2DA;
_PORTE        = 0x2DA;
_PORTEbits    = 0x2DA;
 LATE         = 0x2DC;
_LATE         = 0x2DC;
_LATEbits     = 0x2DC;
 TRISF        = 0x2DE;
_TRISF        = 0x2DE;
_TRISFbits    = 0x2DE;
 PORTF        = 0x2E0;
_PORTF        = 0x2E0;
_PORTFbits    = 0x2E0;
 LATF         = 0x2E2;
_LATF         = 0x2E2;
_LATFbits     = 0x2E2;
 TRISG        = 0x2E4;
_TRISG        = 0x2E4;
_TRISGbits    = 0x2E4;
 PORTG        = 0x2E6;
_PORTG        = 0x2E6;
_PORTGbits    = 0x2E6;
 LATG         = 0x2E8;
_LATG         = 0x2E8;
_LATGbits     = 0x2E8;
 PADCFG1      = 0x2FC;
_PADCFG1      = 0x2FC;
_PADCFG1bits  = 0x2FC;
 ADC1BUF0     = 0x300;
_ADC1BUF0     = 0x300;
 ADC1BUF1     = 0x302;
_ADC1BUF1     = 0x302;
 ADC1BUF2     = 0x304;
_ADC1BUF2     = 0x304;
 ADC1BUF3     = 0x306;
_ADC1BUF3     = 0x306;
 ADC1BUF4     = 0x308;
_ADC1BUF4     = 0x308;
 ADC1BUF5     = 0x30A;
_ADC1BUF5     = 0x30A;
 ADC1BUF6     = 0x30C;
_ADC1BUF6     = 0x30C;
 ADC1BUF7     = 0x30E;
_ADC1BUF7     = 0x30E;
 ADC1BUF8     = 0x310;
_ADC1BUF8     = 0x310;
 ADC1BUF9     = 0x312;
_ADC1BUF9     = 0x312;
 ADC1BUFA     = 0x314;
_ADC1BUFA     = 0x314;
 ADC1BUFB     = 0x316;
_ADC1BUFB     = 0x316;
 ADC1BUFC     = 0x318;
_ADC1BUFC     = 0x318;
 ADC1BUFD     = 0x31A;
_ADC1BUFD     = 0x31A;
 ADC1BUFE     = 0x31C;
_ADC1BUFE     = 0x31C;
 ADC1BUFF     = 0x31E;
_ADC1BUFF     = 0x31E;
 AD1CON1      = 0x320;
_AD1CON1      = 0x320;
_AD1CON1bits  = 0x320;
 AD1CON2      = 0x322;
_AD1CON2      = 0x322;
_AD1CON2bits  = 0x322;
 AD1CON3      = 0x324;
_AD1CON3      = 0x324;
_AD1CON3bits  = 0x324;
 AD1CHS       = 0x328;
_AD1CHS       = 0x328;
_AD1CHSbits   = 0x328;
 AD1PCFG      = 0x32C;
_AD1PCFG      = 0x32C;
_AD1PCFGbits  = 0x32C;
 AD1CSSL      = 0x330;
_AD1CSSL      = 0x330;
_AD1CSSLbits  = 0x330;
 PMCON        = 0x600;
_PMCON        = 0x600;
_PMCONbits    = 0x600;
 PMMODE       = 0x602;
_PMMODE       = 0x602;
_PMMODEbits   = 0x602;
 PMADDR       = 0x604;
_PMADDR       = 0x604;
_PMADDRbits   = 0x604;
 PMDOUT1      = 0x604;
_PMDOUT1      = 0x604;
 PMDOUT2      = 0x606;
_PMDOUT2      = 0x606;
 PMDIN1       = 0x608;
_PMDIN1       = 0x608;
 PMDIN2       = 0x60A;
_PMDIN2       = 0x60A;
 PMPEN        = 0x60C;
_PMPEN        = 0x60C;
_PMPENbits    = 0x60C;
 PMSTAT       = 0x60E;
_PMSTAT       = 0x60E;
_PMSTATbits   = 0x60E;
 ALRMVAL      = 0x620;
_ALRMVAL      = 0x620;
 ALCFGRPT     = 0x622;
_ALCFGRPT     = 0x622;
_ALCFGRPTbits = 0x622;
 RTCVAL       = 0x624;
_RTCVAL       = 0x624;
 RCFGCAL      = 0x626;
_RCFGCAL      = 0x626;
_RCFGCALbits  = 0x626;
 CMCON        = 0x630;
_CMCON        = 0x630;
_CMCONbits    = 0x630;
 CVRCON       = 0x632;
_CVRCON       = 0x632;
_CVRCONbits   = 0x632;
 CRCCON       = 0x640;
_CRCCON       = 0x640;
_CRCCONbits   = 0x640;
 CRCXOR       = 0x642;
_CRCXOR       = 0x642;
 CRCDAT       = 0x644;
_CRCDAT       = 0x644;
 CRCWDAT      = 0x646;
_CRCWDAT      = 0x646;
 ODCA         = 0x6C0;
_ODCA         = 0x6C0;
_ODCAbits     = 0x6C0;
 ODCB         = 0x6C6;
_ODCB         = 0x6C6;
_ODCBbits     = 0x6C6;
 ODCC         = 0x6CC;
_ODCC         = 0x6CC;
_ODCCbits     = 0x6CC;
 ODCD         = 0x6D2;
_ODCD         = 0x6D2;
_ODCDbits     = 0x6D2;
 ODCE         = 0x6D8;
_ODCE         = 0x6D8;
_ODCEbits     = 0x6D8;
 ODCF         = 0x6DE;
_ODCF         = 0x6DE;
_ODCFbits     = 0x6DE;
 ODCG         = 0x6E4;
_ODCG         = 0x6E4;
_ODCGbits     = 0x6E4;
 RCON         = 0x740;
_RCON         = 0x740;
_RCONbits     = 0x740;
 OSCCON       = 0x742;
_OSCCON       = 0x742;
_OSCCONbits   = 0x742;
 CLKDIV       = 0x744;
_CLKDIV       = 0x744;
_CLKDIVbits   = 0x744;
 OSCTUN       = 0x748;
_OSCTUN       = 0x748;
_OSCTUNbits   = 0x748;
 NVMCON       = 0x760;
_NVMCON       = 0x760;
_NVMCONbits   = 0x760;
 NVMKEY       = 0x766;
_NVMKEY       = 0x766;
 PMD1         = 0x770;
_PMD1         = 0x770;
_PMD1bits     = 0x770;
 PMD2         = 0x772;
_PMD2         = 0x772;
_PMD2bits     = 0x772;
 PMD3         = 0x774;
_PMD3         = 0x774;
_PMD3bits     = 0x774;
