### uVision2 Project, (C) Keil Software
### Do not modify !

Target (LM3S1xx), 0x0004 // Tools: 'ARM-ADS'

Group (Source)
Group (Demo)

File 1,1,<..\..\Source\croutine.c><croutine.c>
File 1,1,<..\..\Source\list.c><list.c>
File 1,1,<..\..\Source\queue.c><queue.c>
File 1,1,<..\..\Source\tasks.c><tasks.c>
File 1,1,<..\..\Source\portable\MemMang\heap_1.c><heap_1.c>
File 1,1,<..\..\Source\portable\RVDS\ARM_CM3\port.c><port.c>
File 2,1,<.\main.c><main.c>
File 2,2,<.\init\Startup.s><Startup.s>
File 2,1,<..\Common\Minimal\crflash.c><crflash.c>
File 2,1,<.\ParTest\ParTest.c><ParTest.c>
File 2,1,<.\include\pdc.c><pdc.c>
File 2,4,<..\Common\drivers\LuminaryMicro\Keil\driverlib.lib><driverlib.lib>


Options 1,0,0  // Target 'LM3S1xx'
 Device (LM3S101)
 Vendor (Luminary Micro)
 Cpu (IRAM(0x20000000-0x200007FF) IROM(0-0x1FFF) CLOCK(20000000) CPUTYPE("Cortex-M3"))
 FlashUt ()
 StupF ("STARTUP\Luminary\Startup.s" ("Luminary Startup Code"))
 FlashDR (UL2CM3(-U40296420 -O7 -S0 -C0 -FO7 -FD20000000 -FC800 -FN1 -FF0LM3S_8 -FS00 -FL02000))
 DevID (4079)
 Rgf (LM3Sxxx.H)
 Mem ()
 C ()
 A ()
 RL ()
 OH ()
 DBC_IFX ()
 DBC_CMS ()
 DBC_AMS ()
 DBC_LMS ()
 UseEnv=0
 EnvBin ()
 EnvInc ()
 EnvLib ()
 EnvReg (˙Luminary\)
 OrgReg (˙Luminary\)
 TgStat=16
 OutDir (.\uvision\)
 OutName (RTOSDemo)
 GenApp=1
 GenLib=0
 GenHex=0
 Debug=1
 Browse=1
 LstDir (.\uvision\)
 HexSel=1
 MG32K=0
 TGMORE=0
 RunUsr 0 0 <>
 RunUsr 1 0 <>
 BrunUsr 0 0 <>
 BrunUsr 1 0 <>
 CrunUsr 0 0 <>
 CrunUsr 1 0 <>
 SVCSID <>
 GLFLAGS=1790
 ADSFLGA { 243,31,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ACPUTYP ("Cortex-M3")
 RVDEV ()
 ADSTFLGA { 0,12,0,2,99,0,0,66,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCMADSOCM { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCMADSIRAM { 0,0,0,0,32,0,8,0,0 }
 OCMADSIROM { 1,0,0,0,0,0,32,0,0 }
 OCMADSXRAM { 0,0,0,0,0,0,0,0,0 }
 OCR_RVCT { 1,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,0,0,32,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,32,0,8,0,0,0,0,0,0,0,0,0,0,0 }
 RV_STAVEC ()
 ADSCCFLG { 8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSCMISC ()
 ADSCDEFN (RVDS_ARMCM3_LM3S102)
 ADSCUDEF ()
 ADSCINCD (C:\Keil\ARM\RV30\LIB\Luminary;..\CORTEX_LM3S102_KEIL;..\..\Source\portable\RVDS\ARM_CM3;..\..\Source\include;..\Common\include;.\include)
 ADSASFLG { 65,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSAMISC (--diag_suppress 1581)
 ADSADEFN ()
 ADSAUDEF ()
 ADSAINCD ()
 PropFld { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IncBld=1
 AlwaysBuild=0
 GenAsm=0
 AsmAsm=0
 PublicsOnly=0
 StopCode=3
 CustArgs ()
 LibMods ()
 ADSLDFG { 16,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSLDTA (0x00000000)
 ADSLDDA (0x20000000)
 ADSLDSC ()
 ADSLDIB ()
 ADSLDIC ()
 ADSLDMC (--entry Reset_Handler)
 ADSLDIF ()
 ADSLDDW (6306)
  OPTDL (SARMCM3.DLL)()(DLM.DLL)(-pLM3S101)(SARMCM3.DLL)()(TLM.DLL)(-pLM3S101)
  OPTDBG 49150,1,()()()()()()()()()() (BIN\UL2CM3.DLL)()()()
 FLASH1 { 1,0,0,0,1,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0 }
 FLASH2 (BIN\UL2CM3.DLL)
 FLASH3 ("" ())
 FLASH4 ()
EndOpt

